Recycling Input Characterisation Guidelines: PE Films

|  |  |
| --- | --- |
| Characteristics | Description |
| Resin | [ ]  PE-LD | [ ]  PE-LLD | [ ]  PE-HD |
| Product | Click or tap here to enter text. |
| Origin | Click or tap here to enter text. |
| Source | Click or tap here to enter text. |
| Colour | Click or tap here to enter text. |
| PE-LD content (min %) | Click or tap here to enter text. |
| PE-LLD content (min %) | Click or tap here to enter text. |
| PE-HD content (min %) | Click or tap here to enter text. |
| Impurities |  |
| Impurities content (max %) | Click or tap here to enter text. |
|  Metals (max %) | Click or tap here to enter text. |
|  Paper/Cardboard (max %) | Click or tap here to enter text. |
|  PVC (max %) | Click or tap here to enter text. |
|  PP (max %) | Click or tap here to enter text. |
|  Other plastics (max %) | Click or tap here to enter text. |
| Moisture (max %) | Click or tap here to enter text. |
| Prohibited impurities | Hazardous waste, Medical waste, Glass, Minerals, Oxo- or degradable material, Food contamination, Silicone, EPS & PUR |
| Transport | Stable and stackable bales |
| Transport/contract documents | The documents will be provided with the bales |
| Truck load (min, tonne) | Click or tap here to enter text. |
| Bale characterisations |  |
| Bale size/weight | Click or tap here to enter text. |
| Strapping | Click or tap here to enter text. |

|  |  |
| --- | --- |
| Supplier information |  |
| Company name | Click or tap here to enter text. |
| Company address | Click or tap here to enter text. |
| Additional sorting information | Click or tap here to enter text. |
| Date | Click or tap here to enter text. |

**Glossary**

* **Product**: Stretch film (< 20µm), Shrink film (< 20µm), Pellet covers (20µm < x < 90µm), Thin film (< 90µm), Thick film (> 90µm)
* **Origin**: Commercial & Industrial Waste, Household Waste, Agricultural Waste
* **Source**: Agriculture, Building & Construction, Packaging – Household, Packaging - Transport & Industry, “Housewares, Leisure, Sports etc”, Others (specify).
* **Colour**:
	+ Transparent natural share versus coloured: 98/2%, 90/10%, 80/20%, 70/30%, 60/40% and 50/50%, 40/50%, 30/70%, 20/80%, 10/90% & 2/98%.
	+ Black or white farm film
* **Impurities content**: the impurities content is the sum of all the unwanted impurities.
* **Prohibited Impurities**: the listed prohibited impurities should not be present in the bales.
* **Bale strapping**: indicate the type of strapping used; steel wires are the preferred option