Recycled PP Pellets Characteristics

|  |  |
| --- | --- |
| Characteristics | Description |
| Product name | Click or tap here to enter text. |
| Product reference | Click or tap here to enter text. |
| Applications | Click or tap here to enter text. |
| Origin of the materials | Click or tap here to enter text. |
| Colour | Click or tap here to enter text. |
| Technical Properties | Value | Unit | Test method |
| Density | Click or tap here to enter text. | g/cm3 or kg/m3 | EN ISO 1183-1:2019 |
| Bulk density | Click or tap here to enter text. | g/cm3 or kg/m3 | ISO 60 or EN 15345 |
| Melt flow rate | Click or tap here to enter text. | g/10min | EN ISO 1133-1:2011 |
| Ash content | Click or tap here to enter text. | weight % | EN ISO 3451-1:2019 |
| Filtration | Click or tap here to enter text. | µm | Internal method |
| Moisture | Click or tap here to enter text. | weight % | Moisture Analyser / infrared heater or TGA EN ISO 11358-1:2014 |
| Impurities | Click or tap here to enter text. |  | Visual inspection |
| Appearance | Click or tap here to enter text. |  | Visual inspection |
| Transport |  |
| Packaging | Click or tap here to enter text. |
| Transport/contract documents | The document(s) will be provided with the product. |
| Truck load | Click or tap here to enter text. |

|  |  |
| --- | --- |
| Supplier information |  |
| Company name | Click or tap here to enter text. |
| Company address | Click or tap here to enter text. |
| Date | Click or tap here to enter text. |

**Glossary**

* Origin: Post-consumer and/or Pre-consumer
* Colour: Transparent, translucent, light dark or other
* Filtration: Indicate the filter used during extrusion in µm
* Impurities: describe the impurities visible in the pellet
* Appearance: describe the shape of the pellet and if it has a normal shiny and smooth appearance